Bone Springs Victoria Peak V1.01 Groundwater Availability Model Boundary Condition Packages. 
Texas Water Development Board Groundwater Modeling Department

********************************************************************************************************************
WEL - WELL PKG
bsvp_v101_wel.csv
bsvp_v101_bc_pkg.gpkg\bsvp_v101_wel
********************************************************************************************************************
cellid 	| integer 	| Format:  layer + rrrr + cccc (0-3 leading zeros for row and cols). Example: 200230245 (layer = 2, row = 23, col = 245)
lay 	| integer 	| Layer number
row 	| integer 	| Row number 
col 	| integer 	| Column number
ibound 	| integer 	| ibound number
q1	 	| float 	| pumping for stress period 1
qN 		| float 	| pumping for stress period N
**********************************************************************************************************************
DRN - DRN PKG
bsvp_v101_drn.csv
bsvp_v101_bc_pkg.gpkg\bsvp_v101_drn
********************************************************************************************************************
cellid 	| integer 	| Format:  layer + rrrr + cccc (0-3 leading zeros for row and cols). Example: 200230245 (layer = 2, row = 23, col = 245)
lay 	| integer 	| Layer number
row 	| integer 	| Row number 
col 	| integer 	| Column number
ibound 	| integer 	| ibound number
elev	| float 	| drain elevation for all Stress Periods
cond	| float 	| drain conductivity for all Stress Periods
**********************************************************************************************************************
GHB - GENERAL HEAD BOUNDARY PKG
bsvp_v101_ghb.csv
bsvp_v101_bc_pkg.gpkg\bsvp_v101_ghb
********************************************************************************************************************
cellid 	| integer 	| Format:  layer + rrrr + cccc (0-3 leading zeros for row and cols). Example: 200230245 (layer = 2, row = 23, col = 245)
lay 	| integer 	| Layer number
row 	| integer 	| Row number 
col 	| integer 	| Column number
ibound 	| integer 	| ibound number
cond 	| float 	| hydraulic conductance of the interface between the aquifer cell and the boundary for all stress periods
head	| float		| ghb cell head in feet for all stress periods
**********************************************************************************************************************
RCH - RECHARGE PKG
bsvp_v101_rch.csv
bsvp_v101_bc_pkg.gpkg\bsvp_v101_rch
********************************************************************************************************************
cellid 	| integer 	| Format:  layer + rrrr + cccc (0-3 leading zeros for row and cols). Example: 200230245 (layer = 2, row = 23, col = 245)
lay 	| integer 	| Layer number
row 	| integer 	| Row number 
col 	| integer 	| Column number
ibound 	| integer 	| ibound number
rech1	| float 	| recharge for stress period 1
rechN	| float 	| recharge for stress period N
**********************************************************************************************************************
RIV - RIVER PKG
bsvp_v101_riv.csv
bsvp_v101_bc_pkg.gpkg\bsvp_v101_riv
********************************************************************************************************************
cellid 	| integer 	| Format:  layer + rrrr + cccc (0-3 leading zeros for row and cols). Example: 200230245 (layer = 2, row = 23, col = 245)
lay 	| integer 	| Layer number
row 	| integer 	| Row number 
col 	| integer 	| Column number
ibound 	| integer 	| ibound number
rbot	| float		| elevation of the bottom of the riverbed for all Stress Periods
cond	| float 	| riverbed hydraulic conductance for all Stress Periods
stage1	| float 	| head in the river cell for SP 1
stageN	| float 	| head in the river cell for SP N
**********************************************************************************************************************
CHD - CONSTANT HEAD PKG
bsvp_v101_chd.csv
bsvp_v101_bc_pkg.gpkg\bsvp_v101_chd
********************************************************************************************************************
cellid 	| integer 	| Format:  layer + rrrr + cccc (0-3 leading zeros for row and cols). Example: 200230245 (layer = 2, row = 23, col = 245)
lay 	| integer 	| Layer number
row 	| integer 	| Row number 
col 	| integer 	| Column number
ibound 	| integer 	| ibound number
shead1	| float		| is the head at the boundary at the start of the stress period 1
sheadN	| float 	| is the head at the boundary at the start of the stress period N
ehead1	| float 	| is the head at the boundary at the end of the stress period 1
eheadN	| float 	| is the head at the boundary at the end of the stress period N
**********************************************************************************************************************
HFB - HORIZONTAL FLOW BARRIER PKG
bsvp_v101_hfb.csv
bsvp_v101_bc_pkg.gpkg\bsvp_v101_hfb
********************************************************************************************************************
cellid 	| integer 	| Format:  layer + rrrr + cccc (0-3 leading zeros for row and cols). Example: 200230245 (layer = 2, row = 23, col = 245)
lay 	| integer 	| Layer number
row 	| integer 	| Row number 
col 	| integer 	| Column number
ibound 	| integer 	| ibound number
hydchr	| float		| is the hydraulic characteristic of the horizontal-flow barrier. The hydraulic characteristic is the barrier hydraulic conductivity divided by the width of the horizontal-flow barrier.
**********************************************************************************************************************
EVT - EVAPOTRANSPIRATION PKG
bsvp_v101_evt.csv
bsvp_v101_bc_pkg.gpkg\bsvp_v101_evt
********************************************************************************************************************
cellid 	| integer 	| Format:  layer + rrrr + cccc (0-3 leading zeros for row and cols). Example: 200230245 (layer = 2, row = 23, col = 245)
ievt 	| integer 	| layer number recharge is applied to
row 	| integer 	| Row number 
col 	| integer 	| Column number
ibound | integer 	| ibound number
surf	| float 	| elevation of ET surface for all stress periods
evtr1	| float 	| max ET flux rate for SP 1
evtrN	| float 	| max ET flux rate for SP N
exdp1	| float 	| ET extinction depth for SP 1
exdpN	| float 	| ET extinction depth for SP N
**********************************************************************************************************************
For more information on the variables refer to:
USGS Open-File Report 00-92
MODFLOW-2000, The U.S. Geological Survey Modular Ground-Water Model - User Guide to Modularization Concepts and the Groundwater Flow Process