ebfz_b_v101_flow_props.csv
ebfz_b_v101_flow_props.gpkg

*******************************************************************************************************************
Edwards Balcones Fault Zone - Barton Springs V101 Groundwater Availability Model Flow Properties Grid. 
Texas Water Development Board Groundwater Modeling Department
Only active model cells are included (ibound = 1). Inactive cells (ibound = 0) are not included.

********************************************************************************************************************
cellid 	| integer 	| Format:  layer + rrrr + cccc (0-3 leading zeros for row and cols). Example: 200230245 (layer = 2, row = 23, col = 245)
lay 	| integer 	| Layer number
row 	| integer 	| Row number 
col 	| integer 	| Column number
ibound 	| integer 	| ibound number
top 	| float 	| top of model cell for row and col
bot 	| float 	| bottom of model cell 
shead 	| float 	| the initial (starting) head
hy 		| float 	| hydraulic conductivity along rows
trpy 	| integer 	| one-dimensional array containing an anisotropy factor for each layer.
sf1 	| float 	| primary storage coefficient.
sf2 	| float 	| secondary storage coefficient.
vcont 	| float 	| vertical hydraulic conductivity divided by the thickness from a layer to the layer below.

**********************************************************************************************************************
For more information on the variables ibound, top, bot, shead, hy, trpy, sf1, sf2, and vcont refer to:
USGS Open-File Report 96-485
User's Documentation for MODFLOW-96, an update to the U.S. Geological Survey Modular Finite-Difference Ground-Water Flow Model