eddt_p_v101_alt_flow_props.csv
eddt_p_v101_alt_flow_props.gpkg

*******************************************************************************************************************
Edwards-Trinity (Plateau) Alternative v1.01 Model Groundwater Availability Model Flow Properties Grid. 
Texas Water Development Board Groundwater Modeling Department
Only active model cells are included (ibound = 1). Inactive cells (ibound = 0) are not included.

********************************************************************************************************************
cellid 	| integer 	| Format:  layer + rrrr + cccc (0-3 leading zeros for row and cols). Example: 200230245 (layer = 2, row = 23, col = 245)
lay 	| integer 	| Layer number
row 	| integer 	| Row number 
col 	| integer 	| Column number
ibound 	| integer 	| ibound number
shead	| float		| starting head of the model cell
top 	| float 	| top of model cell
bot 	| float 	| bottom of model cell 
hk		| float		| hydraulic conductivity along rows.
vka		| float		| is either vertical hydraulic conductivity or the ratio of horizontal to vertical hydraulic conductivity 
hani	| float		| ratio of hydraulic conductivity along columns to hydraulic conductivity along rows
ss		| float		| specific storage
sy		| float		| specific yield.

**********************************************************************************************************************
For more information on the variables refer to:
USGS Open-File Report 00-92
MODFLOW-2000, The U.S. Geological Survey Modular Ground-Water Model - User Guide to Modularization Concepts and the Groundwater Flow Process