symr_v101_flow_props.csv
symr_v101_flow_props.gpkg

*******************************************************************************************************************
Seymour/Blaine V1.01 Aquifer Groundwater Availability Model Flow Properties Grid. 
Texas Water Development Board Groundwater Modeling Department
Only active model cells are included (ibound > 0). Inactive cells (ibound = 0) are not included.

********************************************************************************************************************
cellid 	| integer 	| Format:  layer + rrrr + cccc (0-3 leading zeros for row and cols). Example: 200230245 (layer = 2, row = 23, col = 245)
lay 	| integer 	| Layer number
row 	| integer 	| Row number 
col 	| integer 	| Column number
ibound 	| integer 	| ibound number
shead	| float		| starting head of the model cell
top 	| float 	| top of model cell
botm 	| float 	| bottom of model cell 
hy		| float		| hydraulic conductivity along rows.
vcont	| float		| vertical hydraulic conductivity divided by the thickness from a layer to the layer below.
sf1		| float		| primary storage coefficient.
sf2		| float		| secondary storage coefficient.

**********************************************************************************************************************
For more information on the variables refer to:
USGS Open-File Report 00-92
MODFLOW-2000, The U.S. Geological Survey Modular Ground-Water Model - User Guide to Modularization Concepts and the Groundwater Flow Process