ebfz_b_v101_heads.csv
ebfz_b_v101_heads.gpkg

*******************************************************************************************************************
Edwards Balcones Fault Zone V101 Groundwater Availability Model Heads for Historical Model
Texas Water Development Board Groundwater Modeling Department
Only active model cells are included (ibound = 1). Inactive cells (ibound = 0) are not included.

********************************************************************************************************************
cellid	| integer	| Format:  layer + rrrr + cccc (0-3 leading zeros for row and cols), Example: 200230245 (layer = 2, row = 23, col = 245)
lay 	| integer 	| Layer number
row 	| integer 	| Row number 
col 	| integer 	| Column number
ibound 	| integer 	| ibound number
top 	| float 	| top of model cell
bot 	| float 	| bottom of model cell
top		| float		| the elevation of the top of the cell
botm	| float		| the elevation of the bottom of the cell
shead 	| float 	| the initial (starting) head 
head1 	| float 	| head for stress period 1
headN	| float		| head for stress period N

**********************************************************************************************************************
For more information on the variables refer to:
USGS Open-File Report 96-485
User's Documentation for MODFLOW-96, an update to the U.S. Geological Survey Modular Finite-Difference Ground-Water Flow Model